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	Document title
	Weekly Site Inspection Form

	Document reference
	[Document Ref]

	Pack / library
	Pro Site Docs — Weekly Site Inspection Form

	Revision
	[Revision]

	Status
	[Draft / For Review / Approved / Live]

	Issue date
	[Date]

	Review date
	[Review Date]



Pro Site Docs is operated by LDH Pipeline Services Ltd and forms part of the wider LDH Construction Hub ecosystem.


	1   DOCUMENT CONTROL



	Field
	Project-Specific Entry

	Document title
	Weekly Site Inspection Form

	Document number
	[Document Ref]

	Revision
	[Revision]

	Status
	[Draft / For Review / Approved / Live / Closed]

	Project name
	[Project Name]

	Client
	[Client Name]

	Principal contractor
	[Principal Contractor]

	Contractor
	[Contractor]

	Site / location
	[Site Address]

	Prepared by
	[Prepared By]

	Checked by
	[Responsible Person]

	Approved by
	[Approver]

	Issue date
	[Date]

	Review date
	[Review Date]



	2   REVISION HISTORY



	Rev
	Date
	Description of change
	Prepared
	Checked
	Approved

	[Rev]
	[Date]
	Initial issue for project adaptation.
	[Name]
	[Name]
	[Name]

	
	
	
	
	
	

	
	
	
	
	
	



	3   PURPOSE



To provide a controlled record for weekly site inspection, supporting compliance, monitoring and continuous improvement on the project.
	4   SCOPE



This document applies specifically to pipeline works on the project. Weekly documented site inspection at [Project Name] covering the principal health, safety and environmental controls, with actions tracked to close-out.
When to use this document
Use during the works to record and control the activity, and retain the completed record as project evidence for audit, inspection and handover.
Who should complete it
A competent person — typically the Site Manager, Supervisor or relevant discipline lead.
	5   APPLICABLE LEGISLATION & GUIDANCE



▪  Health and Safety at Work etc. Act 1974
▪  Construction (Design and Management) Regulations 2015
▪  Management of Health and Safety at Work Regulations 1999
▪  Personal Protective Equipment at Work Regulations 1992 (as amended 2022)
▪  Reporting of Injuries, Diseases and Dangerous Occurrences Regulations 2013 (RIDDOR)
▪  HSG47 – Avoiding danger from underground services
▪  Lifting Operations and Lifting Equipment Regulations 1998 (LOLER)
▪  Provision and Use of Work Equipment Regulations 1998 (PUWER)
▪  Work at Height Regulations 2005
▪  Control of Substances Hazardous to Health Regulations 2002 (COSHH)
▪  Electricity at Work Regulations 1989
▪  New Roads and Street Works Act 1991
▪  Safety at Street Works and Road Works – A Code of Practice
▪  Railways and Other Guided Transport Systems (Safety) Regulations 2006 (ROGS)
▪  Regulatory Reform (Fire Safety) Order 2005
▪  Dangerous Substances and Explosive Atmospheres Regulations 2002 (DSEAR)
▪  Environmental Protection Act 1990
▪  Environmental Protection (Duty of Care) Regulations 1991
	6   RESPONSIBILITIES



	Role
	Responsibility

	Project / Site Manager
	Owns delivery of this document on site, resourcing, briefing and escalation.

	Supervisor
	Day-to-day supervision, inspection and briefing of operatives.

	Operatives
	Comply with this document and report changes, defects or concerns.



	7   COMPETENCE REQUIREMENTS



	Role
	Competence required
	Evidence

	Site Manager
	SMSTS / SSSTS
	Certificate



	8   PPE REQUIREMENTS



The following minimum PPE applies. Confirm task-specific PPE against the risk assessment before work starts.
▪  Standard site PPE for inspection
	9   PLANT & EQUIPMENT



▪  360° excavator with quick-hitch and certified lifting points
▪  Trench support system (trench box / shoring) to temporary works design
▪  Dewatering pump(s) and hoses
▪  CAT & Genny (cable avoidance tool & signal generator)
▪  Lifting appliance (crane / HIAB / excavator) within rated capacity
▪  Certified lifting accessories (slings, shackles, chains) within SWL
▪  Tag lines, packing and outrigger mats
▪  Access equipment (tower, podium, ladder, edge protection) selected to the task
▪  Fall-arrest equipment with suitable anchors (where used)
▪  Traffic management equipment (signs, cones, barriers, lamps) to the Code of Practice
▪  Road-rail vehicle (RRV) / on-track plant with current examination
▪  Rail trolleys and approved access equipment
▪  All plant and equipment inspected before use and within examination dates (PUWER/LOLER)
	10   MATERIALS



▪  Bedding and selected backfill material to specification
▪  Pipe, fittings and jointing materials as specified
▪  Marker tape / service protection tiles
▪  All materials stored, handled and used in line with the manufacturers’ data sheets and COSHH assessments
	11   CHECKLIST



	Item
	Yes
	No
	N/A
	Comments / action

	Excavations supported, inspected & barriered
	
	
	
	

	Working at height / edge protection
	
	
	
	

	Lifting operations controlled
	
	
	
	

	Plant condition, guards & checks
	
	
	
	

	Electrical / temporary supplies safe
	
	
	
	

	COSHH storage & spill kits
	
	
	
	

	Fire points & emergency routes clear
	
	
	
	

	Welfare & first aid adequate
	
	
	
	

	Traffic management & public protection
	
	
	
	

	Housekeeping & PPE compliance
	
	
	
	

	Permits & RAMS being followed
	
	
	
	



	12   ACTIONS ARISING



	Action
	Owner
	Target date
	Status

	
	
	
	

	
	
	
	



	13   ENVIRONMENTAL CONTROLS



▪  Prevent pollution of drains and watercourses; spill kits available and used
▪  Segregate and dispose of waste under the duty of care; retain transfer notes
▪  Control dust and noise/vibration from the works
▪  Fuel and oils in bunded storage; refuel over drip trays away from drains
	14   EMERGENCY ARRANGEMENTS



In an emergency, stop work, make the area safe, raise the alarm and follow the site emergency procedure. Record the specific arrangements below.
	Scenario
	Action

	Imminent danger found
	Stop the work, make safe, and escalate immediately



	Emergency item
	Project entry

	Emergency contact / number
	[Entry]

	Nearest A&E
	[Hospital / address]

	First aider(s)
	[Name(s)]

	Assembly point
	[Location]

	Site address for 999
	[Site Address]



	15   COMPLETION GUIDANCE



▪  Complete every [bracketed] placeholder with project-specific detail before the document is issued.
▪  Have a competent person review, adapt and approve the document for the specific works.
▪  Brief all affected personnel and record their names and signatures in the sign-off.
▪  Keep the document live — update and re-issue it when the work, site conditions, plant or risks change.
▪  Tie supporting evidence (drawings, manufacturer data, test sheets, permits) into the records where referenced.
	16   MONITORING & REVIEW



	Inspection / check
	Requirement / frequency

	Inspection
	At the required frequency and after change

	Actions
	Tracked to close-out



Findings feed the review of method and controls.
	Review trigger
	Required action
	Owner / evidence

	Change to design, method, plant, site or programme
	Review controls and re-brief before continuing.
	[Owner / Evidence]

	Incident, near miss, failed inspection or client concern
	Stop, make safe, investigate and amend the document if required.
	[Owner / Evidence]

	Scheduled review date reached
	Confirm still suitable or issue a revised version.
	[Owner / Evidence]



	17   APPROVAL & SIGN-OFF



The following confirm they have prepared, checked and approved this document, and that briefed personnel have read, understood and will comply with it.
	Approval role
	Name
	Signature
	Date

	Prepared by
	[Name]
	
	

	Checked by
	[Name]
	
	

	Approved by
	[Name]
	
	

	Client acceptance (where required)
	[Name]
	
	



Briefing record
	Name
	Company / role
	Signature
	Date

	Inspector
	Completed the inspection.
	
	

	Action owners
	Close out actions.
	
	

	
	
	
	

	
	
	
	



	!   DISCLAIMER



This template is provided as an editable construction documentation template and must be reviewed, adapted and approved by a competent person before use. Pro Site Docs and LDH Pipeline Services Ltd do not accept responsibility for documents used without project-specific review, risk assessment or professional judgement. No template is automatically compliant without project-specific adaptation.
Controlled template — complete project-specific details and obtain competent review before issue.   © Pro Site Docs / LDH Pipeline Services Ltd     Page 1 of 1
